DTC B2477

#
DTC B2477

B3E080201046W27

DTC B2477 | Configuration error
--- | ---

DETECTION CONDITION

  Warning

  • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure.

• SAS control module configuration has not been performed correctly.

POSSIBLE CAUSE | • SAS control module configuration error • SAS control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT SAS CONTROL MODULE • Using the WDS or equivalent, perform SAS control module configuration. • Is DTC B2477 indicated? | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.