CENTER PANEL MODULE REMOVAL/INSTALLATION

#
CENTER PANEL MODULE REMOVAL/INSTALLATION

B3E092066900W02

1. Disconnect the negative battery cable.

2. Remove the decoration panel.(See DECORATION PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Antenna feeder
4 | Center panel module (See Center Panel Module Removal Note.)

4. Install in the reverse order of removal.

  Caution

  • When installing the center panel module, make sure that the wiring harness and antenna feeder are not caught between the unit and dashboard.If the wiring harness or the antenna feeder is caught between the unit and dashboard, it may cause malfunctions.

## Center Panel Module Removal Note

1. Pull the center panel module outward, detach clip A from the dashboard, and then remove the center panel module.