FRONT SEAT DISASSEMBLY/ASSEMBLY

#
FRONT SEAT DISASSEMBLY/ASSEMBLY

B3E091357100W02

  Warning

  • Handling the front seat (with a side air bag and a pre-tensioner seat belt) improperly can accidentally deploy the side air bag and pre-tensioner seat belt, which may seriously injure you. Read the service warnings before handling the front seat (with a side air bag and a pre-tensioner seat belt). (See SERVICE WARNINGS.)

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

## Driver's Seat

1 | Headrest
2 | Recliner lever (lever type)/Recliner dial (dial type)
3 | Outer lift lever cover
4 | Lift lever
5 | Inner lift lever cover
6 | Seat cushion frame
7 | Seat cushion trim
8 | Seat cushion pad
9 | Pole guide
10 | Lumbar support lever
11 | Seat back frame
12 | Seat back trim
13 | Seat back pad
14 | Side air bag module (SeeSIDE AIR BAG MODULE REMOVAL/INSTALLATION.)
15 | Side cover
16 | Reverse cover
17 | Front buckle
18 | Slide adjuster

## Passenger's Seat

1 | Headrest
2 | Recliner lever
3 | Seat cushion frame
4 | Seat cushion trim
5 | Seat cushion pad
6 | Pole guide
7 | Seat back frame
8 | Seat back trim
9 | Seat back pad
10 | Side air bag module
11 | Side cover
12 | Reverse cover
13 | Front buckle
14 | Slide adjuster