EMISSION SYSTEM LOCATION INDEX [ZJ, Z6, LF]

#
EMISSION SYSTEM LOCATION INDEX [ZJ, Z6, LF]

B3E011601074W01

## Engine Compartment Side

ZJ, Z6

.

1 | Positive crankcase ventilation (PCV) valve (See POSITIVE CRANKCASE VENTILATION (PCV) VALVE INSPECTION [ZJ, Z6, LF].)
2 | EGR valve (See EGR VALVE REMOVAL/INSTALLATION [ZJ, Z6].) (See EGR VALVE INSPECTION [ZJ, Z6, LF].)
3 | Purge solenoid valve (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [ZJ, Z6].) (See PURGE SOLENOID VALVE INSPECTION [ZJ, Z6, LF].)

LF

.

1 | Positive crankcase ventilation (PCV) valve (See POSITIVE CRANKCASE VENTILATION (PCV) VALVE INSPECTION [ZJ, Z6, LF].)
2 | EGR valve (See EGR VALVE REMOVAL/INSTALLATION [LF].) (See EGR VALVE INSPECTION [ZJ, Z6, LF].)
3 | Purge solenoid valve (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [LF].) (See PURGE SOLENOID VALVE INSPECTION [ZJ, Z6, LF].)

## Fuel Tank Side

.

1 | Charcoal canister (See CHARCOAL CANISTER REMOVAL/INSTALLATION [ZJ, Z6, LF].) (See CHARCOAL CANISTER INSPECTION [ZJ, Z6, LF].)
2 | Rollover valve (See ROLLOVER VALVE REMOVAL/INSTALLATION [ZJ, Z6, LF].) (See ROLLOVER VALVE INSPECTION [ZJ, Z6, LF].)