DTC 07:ER02

#
DTC 07:ER02

B3E090266900W21

DTC 07:Er02 | MD player

DETECTION CONDITION

  Note

  • When error occurs, error message "CHECK MD" is displayed in the LCD.

• Cannot play MD normally or change tracks.

POSSIBLE CAUSE | • Defective MD (scratches or dirt) • MD player malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Play the MD and change tracks. Can tracks be changed? | Yes | Go to Step 3.
No | Cannot change to specific tracks. | Go to the next step.
Cannot change to any track. | Change the MD and try to change tracks again. • If the function is normal, go to Step 3. • If the function is not normal, replace the MD player.
2 | Verify the condition of the MD when the error occurs. Is the MD normal? | Yes | Go to the next step.
No | Repair (remove foreign material, clean) or replace the MD, and go to the next step.
3 | Clear the DTC. Play the MD and change tracks. Is DTC 07: Er02 displayed? | Yes | Replace the MD player.
No | DTC troubleshooting completed.