WINDSHIELD WIPER LINK ASSEMBLY/DISASSEMBLY [R.H.D.]

#
WINDSHIELD WIPER LINK ASSEMBLY/DISASSEMBLY [R.H.D.]

B3E091967340W05

## Disassembly

  Note

  • Do not replace link parts individually. If it is necessary to replace any part, replace the windshield wiper link as a single unit.

## Assembly

1. Assemble in the order indicated in the table.

1 | Main link (See Ball Joint Assembly Note.)
2 | Motor crank (See Ball Joint Assembly Note.)
3 | Wiper link No. 1 (See Ball Joint Assembly Note.)
4 | Wiper link No. 2 (See Ball Joint Assembly Note.) (See Wiper Link No. 2 Assembly Note.)

### Ball Joint Assembly Note

1. Use a clean rag to protect the link and squeeze using pliers.

### Wiper Link No. 2 Assembly Note

1. Assemble the wiper link No. 2 positioned as shown in the figure.