DTC B1014

#
DTC B1014

B3E090201072W04

DTC B1014 | Rain sensor error
--- | ---
DETECTION CONDITION | Rain sensor internal malfunction
POSSIBLE CAUSE | • Rain sensor malfunction • PJB malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT DTC • Clear the DTC from the PJB memory using the WDS or equivalent. • Perform the self-test. (See PJB SELF-TEST.) • Is the same DTC present? | Yes | Replace the rain sensor, then go to the next step. (See RAIN SENSOR REMOVAL/INSTALLATION.)
No | Go to the next step.

2

VERIFY TROUBLESHOOTING COMPLETED
• Make sure to reconnect all disconnected connectors.
• Clear the DTC from the PJB memory using the WDS or equivalent.
• Perform the self-test.
(See PJB SELF-TEST.)
• Is the same DTC present?

Yes

Replace the PJB.
(See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)

No | DTC troubleshooting completed.