DTC B1342

#
DTC B1342

B3E090201072W11

DTC B1342 | ECU is faulted
--- | ---
DETECTION CONDITION | PJB microcomputer malfunction
POSSIBLE CAUSE | • PJB microcomputer malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT DTC • Clear the DTC from the PJB memory using the WDS or equivalent. • Perform the self-test. (See PJB SELF-TEST.) • Is the same DTC present? | Yes | Replace the PJB. (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.