CAR-NAVIGATION CONTROL SWITCH REMOVAL/INSTALLATION

#
CAR-NAVIGATION CONTROL SWITCH REMOVAL/INSTALLATION

B3E092066921W01

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Car-navigation control switch (See Car-Navigation Control Switch Removal Note.)
2 | Connector

3. Install in the reverse order of removal.

## Car-Navigation Control Switch Removal Note

1. Pry the car-navigation control switch from the console using a flathead screwdriver wrapped with protective tape.