#
FRONT CROSSMEMBER CONSTRUCTION

BHE021334800T01

• A lightweight, highly rigid front crossmember with integrated side members has been adopted.

• The transverse member is attached to the back of the front crossmember to create a highly rigid square construction.

• This front crossmember component is rigidly mounted to the vehicle body at eight points, providing an extremely large amount of suspension support stiffness and alignment precision.

1 | Side member
2 | Transverse member