#
BALANCE WEIGHT, COUNTERWEIGHT (AT), FLYWHEEL (MT) CONSTRUCTION

BHE011011901T04

• A balance weight and a counterweight (AT) have been installed to prevent dynamic unbalance.

• For MT, a weight has been added to perimeter of the flywheel to obtain the same balancing effect as the counterweight on AT.

• The weight of balance weights for both MT and AT changes in accordance with the difference in rotation-related mass of the transmission that is employed.

1 | MT
2 | Balance weight
3 | Weight
4 | Flywheel
5 | AT
6 | Counterweight