#
DTC B1342 [INSTRUMENT CLUSTER]

BHE090255430W08

DTC B1342 | • Instrument cluster malfunction
--- | ---
DETECTION CONDITION | • Malfunction in the Instrument cluster internal circuit
POSSIBLE CAUSE | • Instrument cluster malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT INSTRUMENT CLUSTER • Clear DTC from memory. • Turn the ignition switch to the LOCK position. • Turn the ignition switch to the ON position. • Is B1342 displayed? | Yes | Replace the instrument cluster.
No | DTC troubleshooting completed.