#
SLOPE MODE CONTROL OPERATION

BHE051318901T19

## When climbing hill

• When the hill is steeper than a certain grade, unnecessary shift up is prevented by holding an appropriate shift gear.

## Descending hill

• When the descent is steeper than a certain grade and the brake switch is depressed, use of the brake pedal is reduced by shifting from 4GR to 3GR, or 3GR to 2GR and applying engine braking.