#
CONDENSER CONSTRUCTION

BHE071161480T02

• A sub cool condenser has been adopted. It is a multi-flow condenser which is equipped with a sub cooling part and integrated with a receiver/drier.

• The sub cool condenser separates liquid-gas refrigerant initially cooled at the condenser via the receiver/drier, where it returns again to the condenser sub cooling part and is cooled, accelerating liquefaction and improving cooling capacity.

1 | Condenser
2 | Receiver/drier
3 | Refrigerant flow
4 | Cooling part
5 | Sub cooling part
6 | IN
7 | OUT