#
EVAPORATIVE EMISSION (EVAP) CONTROL SYSTEM LOCATION INDEX

BHE011601074W01

Engine Compartment Side

1 | Purge solenoid valve (See PURGE SOLENOID VALVE INSPECTION.)
2 | Catch tank (See CATCH TANK INSPECTION.)
3 | AIR control valve (See SECONDARY AIR INJECTION (AIR) CONTROL VALVE REMOVAL/INSTALLATION.) (See SECONDARY AIR INJECTION (AIR) CONTROL VALVE INSPECTION.)
4 | AIR solenoid valve (See SECONDARY AIR INJECTION (AIR) SOLENOID VALVE REMOVAL/INSTALLATION.) (See SECONDARY AIR INJECTION (AIR) SOLENOID VALVE INSPECTION.
5 | AIR pump (See SECONDARY AIR INJECTION (AIR) PUMP REMOVAL/INSTALLATION.) (See SECONDARY AIR INJECTION (AIR) PUMP INSPECTION.)
6 | AIR pump relay (See RELAY INSPECTION.)

Fuel Tank Side

1 | Charcoal canister (See CHARCOAL CANISTER REMOVAL/INSTALLATION.) (See CHARCOAL CANISTER INSPECTION.)
2 | Evaporative chamber (See EVAPORATIVE CHAMBER INSPECTION.)
3 | Rollover valve (See ROLLOVER VALVE INSPECTION.)