#
DTC 00:ER03

BHE090266900W15

DTC 00:Er03 | Cassette deck
DETECTION CONDITION | • Base unit detects that reel built into cassette deck does not operate.
POSSIBLE CAUSE | • Defective cassette tape (tape slack, pinched tape in internal cassette deck) • Cassette deck malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Verify condition of the cassette tape when the error occurs. Is the cassette tape normal? | Yes | Go to the next step.
No | Repair (tighten slack, clear pinched tape inside cassette deck) or replace the cassette tape, and go to the next step.
2 | Clear the DTC, and then insert a normal cassette tape. Play the cassette tape for 20 s or more. Is DTC 00: Er03 displayed? | Yes | Replace the cassette deck.
No | DTC troubleshooting completed.