#
CLUCH SPECIFICATIONS

BHE050001030T03

Item | Specifications
--- | ---
Manual transmission type | R15M-D | Y16M-D
Clutch control | Hydraulic
Clutch cover | Spring type | Diaphragm
Set load | (N {kgf, lbf}) | 5,800 {591, 1304} | 6,470 {660, 1,455}
Clutch disc | Outer diameter | (mm {in}) | 225 {8.86} | 236 {9.29}
Inner diameter | (mm {in}) | 155 {6.10} | 160 {6.30}
Clutch pedal | Type | Suspended
Pedal ratio | 5.7
Full stroke | (mm {in}) | 130 {5.118}
Clutch master cylinder inner diameter | (mm {in}) | 15.87 {0.6248}
Clutch release cylinder inner diameter | (mm {in}) | 19.05 {0.7500}
Clutch fluid type | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT-3 or DOT-4 Australian specs.: SAE J1703, FMVSS 116 DOT-3