#
INSTRUMENTATION/DRIVER INFO. LOCATION INDEX

BHE092201067W01

1 | Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION) (See INSTRUMENT CLUSTER DISASSEMBLY/ASSEMBLY) (See INSTRUMENT CLUSTER INSPECTION) (See INSTRUMENT CLUSTER INPUT/OUTPUT CHECK MODE)
2 | Information display (See INFORMATION DISPLAY REMOVAL/INSTALLATION)
3 | Horn (See HORN REMOVAL/INSTALLATION)
4 | Coolant level switch (See COOLANT LEVEL SWITCH INSPECTION)
5 | Oil pressure switch (See OIL PRESSURE SWITCH INSPECTION)
6 | Oil level switch (See OIL LEVEL SWITCH INSPECTION)
7 | Fuel gauge sender unit (See FUEL GAUGE SENDER UNIT INSPECTION)