#
NO.5 VEHICLE MOVES IN P POSITION, OR PARKING GEAR DOES NOT DISENGAGE WHEN SHIFTED OUT OF P POSITION

BHE050301026W10

5 | Vehicle moves in P position, or parking gear does not disengage when shifted out of P position
DESCRIPTION | • Vehicle rolls on a downward slope in P position. • Tires lock when shifted out of P position. Vehicle does not move in D range and R position when accelerator pedal is depressed, and engine remains in stall condition.
POSSIBLE CAUSE | • Parking mechanism malfunction (May have effect on noise or shock from transmission) • Improper adjustment of selector lever • If vehicle moves in N position, perform No.4 "VEHICLE MOVES IN N POSITION"