#
POWER WINDOW SYSTEM WIRING DIAGRAM

BHE091258000T03

1 | Hall effect switch No. 1
2 | Hall effect switch No. 2
3 | Power window main switch
4 | Power-cut switch
5 | Power window motor (driver's side)
6 | Power window motor (passenger's side)
7 | Power window subswitch
8 | Manual close
9 | Manual open
10 | Auto
11 | Close relay
12 | Open relay
13 | Open
14 | Close
15 | Door switch (driver's side)
16 | Door switch (passenger's side)
17 | Rear door upper latch switch
18 | Rear door lower latch switch
19 | Instrument cluster