#
VANITY MIRROR ILLUMINATION BULB REMOVAL/INSTALLATION

BHE091869270W01

1. Disconnect the negative battery cable.

2. Remove the lens. (See Lens Removal Note.)

3. Remove the vanity mirror illumination bulb.

4. Install in the reverse order of removal.

## Lens Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole and pry with the screwdriver in the direction shown by the arrow to remove the lens.