#
FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION

BHE041543720W01

  Note

  • If there is any malfunction in the front ABS wheel-speed sensor unit, replace the wheel hub component. (See WHEEL HUB, STEERING KNUCKLE REMOVAL/INSTALLATION.)

1. Remove the mudguard.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Connector
2 | Bolt
3 | Front ABS wheel-speed sensor wiring harness