#
RADIATOR CONSTRUCTION

BHE011201008T05

• A corrugated fin type radiator has been adopted.

1 | Tank
2 | Core

• The radiator tanks are made of plastic and the core is made of aluminum for weight reduction.

• The down-flow direction of water inside the radiator causes air to bleed from the cooling system easier.

• Four rubber-insulated mounting brackets are utilized to decrease vibration.

• To improve both the cooling ability and the sporty design, the radiator is designed to tilt forward to reduce the height and to take in the air from the inlet installed under the bumper.