#
OVER-REVOLUTION WARNING ALARM CONSTRUCTION/OPERATION

BHE092255430T10

## System Wiring Diagram

1 | Instrument cluster
2 | Microcomputer
3 | Buzzer
4 | CAN control circuit
5 | PCM
6 | AND

## Operation

• The buzzer in the instrument cluster sounds continuously when both the following two conditions are met:

  – The ignition switch is in ON position.
  – The engine speed is 8,500 rpm or more (13B-MSP (High Power)) or 7,300 rpm or more (13B-MSP (Standard Power)).