#
RELAY INSPECTION

BHE092167730W02

## Relay type

Terminal type | Part name
4 terminals | Type A | • Main relay • TNS relay • ACC relay • Front fog light relay • Drive-by-wire relay • Cooling fan relay No.1 • Cooling fan relay No.2 • A/C relay • Blower relay • Rear window defroster relay • Fuel pump relay • Fuel pump speed control relay • Horn relay • Trunk lid opener relay • Seat warmer relay • Rear fog light relay
Type B | • Ignition relay • Starter relay • Headlight relay • AIR pump relay
5 terminals | Type C | Cooling fan relay No.3

## Type A

1. Verify the continuity between the relay terminals.

  • If not as indicated in the table, replace the relay.

## Type B

1. Verify the continuity between the relay terminals.

  • If not as indicated in the table, replace the relay.

## Type C

1. Verify the continuity between the relay terminals.

  • If not as indicated in the table, replace the relay.