#
FUEL SYSTEM OUTLINE

BHE011401006T01

## Features

Improved serviceability | • Nylon tubes adopted for fuel hoses in the engine compartment and around the fuel tank, and quick release connectors adopted for joints
Reduction of evaporative gas | • Returnless fuel system adopted

## Specification

Item | Specification
--- | ---
Injector | Type | Multiple hole design
Type of fuel delivery | Top-feed
Type of drive | Electronic
Pressure regulator control pressure | (kPa {kgf/cm2, psi}) | Approx. 390 {3.98, 56.6}
Fuel pump type | Electric
Fuel tank capacity | (L {US gal, lmp gal}) | 61 {16.1, 13.4}
Fuel type | Unleaded premium (unleaded high-octane) gasoline