#
ON-BOARD DIAGNOSTIC SYSTEM OUTLINE

BHE070261190T01

## Features

• Includes the on-board diagnostic function and A/C operation check mode. The on-board diagnostic function consists of a malfunction detection function that detects abnormalities in input/ouput signals, a memory function that stores detected malfunctions, a fail-safe function that prevents mis-operation of output parts where a malfunction is detected, and a malfunction display function that displays detected malfunctions.