#
BRAKE SWITCH INSPECTION

BHE041166490W01

  Caution

  • If the brake switch is removed from the brake pedal or the interlock unit, its proper functioning cannot be guaranteed when reinstalled. Therefore, inspect the brake switch with it still installed, or replace the brake switch if it is removed.

1. Verify continuity as indicated in the table.

  • If not as indicated in the table, replace the brake switch.