#
AT WARNING LIGHT CONSTRUCTION/OPERATION

BHE051321101T02

• The AT warning light is built into the instrument cluster.

• The AT warning light illuminates when the instrument cluster receives a warning signal from the PCM via CAN communication.

• The PCM sends a warning signal to the instrument cluster via CAN communication when it detects a malfunction.

1 | Instrument cluster
2 | AT warning light