#
DTC B2477

BHE090255430W09

DTC B2477 | • Configuration error
--- | ---
DETECTION CONDITION | • Configuration error • Malfunction in the instrument cluster internal circuit
POSSIBLE CAUSE | • Instrument cluster malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | PERFORM INSTRUMENT CLUSTER CONFIGURATION • Perform instrument cluster configuration. • Is B2477 displayed? | Yes | Replace the instrument cluster.
No | Go to next step.
2 | VERIFY TROUBLESHOOTING OF DTC B2477 COMPLETED • Clear DTC from memory. • Is B2477 displayed? | Yes | Go to applicable DTC inspection.
No | DTC troubleshooting completed.