#
DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM]

BHE090255430W02

DTC | Malfunction location | DTC output module | Page
--- | --- | --- | ---
U0073 | CAN system communication error | • PCM • TCM • EPS control module • Keyless unit | (See DTC U0073, U1900, U2516)
U0100 | Communication error to PCM | TCM | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION)
U0101 | Communication error to TCM | PCM
U0121 | Communication error to DSC HU/CM
U0155 | Communication error to instrument cluster
U2510 | Communication error to PCM | Keyless unit
U1147
U1900 | CAN system communication error | • DSC HU/CM • EPS control module • Steering angle sensor • Keyless unit • Instrument cluster | (See DTC U0073, U1900, U2516)
U2516 | CAN system wiring harness open or short circuit | • DSC HU/CM • Steering angle sensor • Instrument cluster