#
SYMPTOM TROUBLESHOOTING CHART

BHE090369000W03

No. | Troubleshooting item | Description
--- | --- | ---
1 | One or more on-board diagnostic functions inoperative | • Malfunction in trunk lid opener system, hazard warning light system, or door lock linkage system
2 | All on-board diagnostic functions inoperative | • Malfunction in keyless unit power supply circuit, door switch circuit, or keyless unit ground circuit
3 | Transmitter ID code cannot be reprogrammed | • Malfunction in transmitter battery, transmitter, keyless receiver bracket, keyless receiver bracket ground screw, or keyless unit circuit