#
COMPONENT PART AND FUNCTION

BHE092066000T05

Item | Function
Car-navigation unit | • Reads the data (map, voice and other) from the DVD-ROM. • Calculates and displays the vehicle's position from various signals. • Calculates the route to the destination. • Navigates the driver to the destination using the map screen and/or the voice. Note • DVD audio and video are not supported by this system. • This unit does not support all Video CD and CD formats.
LCD unit | • Displays the screen (menus, maps and other screens) by remote control operation. • Displays the status of audio, DIS and A/C by button operation on the information display.
GPS antenna | • Receives GPS signal from satellites.
Gyro sensor (inside of the car-navigation unit) | • Sends yaw-rate signal to the CPU in the car-navigation unit.
TR switch (AT) or back-up light switch (MT) | • Sends R-range or reverse signal to the car-navigation unit.
DSC HU/CM | • Sends vehicle speed signal to the car-navigation unit by CAN system.
Front speaker and tweeter (driver side) | • Outputs voice and audio sound.
DVD-ROM (inside of the car-navigation unit) | • Map information data of each country is recorded. • Voice data used to guide the route is recorded. • Route information data to search for the route is recorded.
Car-navigation control switch | • Changes display screens, settings etc., by button operation.