#
NO.13 SHIFT POINT IS HIGH OR LOW

BHE050301026W18

13 | Shift point is high or low
DESCRIPTION | • Shift point is considerably different from automatic shift diagram. • Shift delays when accelerating. • Shift occurs suddenly when accelerating and engine speed does not increase.
POSSIBLE CAUSE | • If the transmission shifts normally, there is a malfunction of the input signal to the TP sensor or VSS. • If the engine speed is high or low regardless normal shifting, inspect the tachometer. • Verify that the output signal of the TP sensor changes linearly.