#
MONITORING SYSTEM AND CONTROL SYSTEM DEVICE RELATIONSHIP CHART

BHE010200102W02
×: Applicable

Component |  |  |  |  |  |
--- | --- | --- | --- | --- | --- | ---
Input
Battery |  | × |  | × |  |
Ignition switch | × | × |  |  |  |
TP sensor | × |  | × | × |  | ×
ECT sensor | × | × | × | × | × | ×
IAT sensor | × | × | × | × | × | ×
MAF sensor | × | × | × | × | × | ×
Front HO2S | × | × | × |  | × | ×
Rear HO2S | × | × | × |  |  | ×
BARO sensor | × | × | × | × |  | ×
Eccentric shaft position sensor | × | × | × | × | × | ×
Fuel gauge sender unit |  |  |  | × |  |
DSC HU/CM |  |  |  | × |  |
Output
Fuel injector |  |  | × |  |  |
Front HO2S heater |  | × |  |  |  |
Rear HO2S heater |  | × |  |  |  |
Purge solenoid valve | × |  | × |  |  | ×
AIR solenoid valve |  |  |  |  | × |
AIR pump relay |  |  |  |  | × |
MIL | × | × | × | × | × | ×