#
NO.23 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN D RANGE, OR IN R POSITION

BHE050301026W28

23 | Noise occurs at idle when vehicle is stopped in D range, or in R position
DESCRIPTION | • Transmission is noisy in driving ranges when vehicle is idling.
POSSIBLE CAUSE | • Malfunctions unrelated to AT: – Abnormal noise from differential – Abnormal noise from propeller shaft – Vibration caused by unbalanced or uneven tires Note • Although the malfunction is basically the same as No.22 "NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN ALL POSITIONS/RANGES", other causes may be selector lever position disparity or TR switch position disparity. • Before following the troubleshooting steps, make sure that the Automatic Transmission On-Board Diagnostic and Automatic Transmission Basic Inspection are conducted. (See BASIC INSPECTION.)