#
FRONT BRAKE (DISC) REMOVAL/INSTALLATION

BHE041133980W02

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, depress the brake pedal a few times, then verify that the brakes do not drag.

1 | Brake hose
2 | Bolt
3 | Caliper (See Caliper Installation Note.)
4 | Disc pad
5 | Shim
6 | Guide plate
7 | Bolt
8 | Mounting support
9 | Screw
10 | Disc plate

## Caliper Installation Note

1. Clean the exposed area of the piston.

2. Install the piston using the SST.

3. Install the caliper.