#
AUDIO SYSTEM SPECIFICATIONS

BHE092001066T04

## Audio Unit

Item | Specification
--- | ---
BOSE | Standard
Rated voltage | (V) | 12
Frequency band | AM | (kHz) | 531-1629 (European (L.H.D. U.K.) specs.) 522-1629 (Australian specs.)
FM | (MHz) | 87.5-108.0
Audio amplifier maximum output power | (W) | External type audio amplifier • Main amplifier – 25×3 – 12.75×2 • Front door speaker amplifier – 100×1 | 25×4
Output impedance | (ohm) | 2 | 4

## Speaker

Item | Specification
--- | ---
Front door speaker | Rear speaker | Tweeter | Center speaker
Standard | BOSE | Standard | BOSE | Front | Rear
Standard* | BOSE
Maximum input | (W) | 25 | 100 | 25 | 37.5 | 25 | 12.5 | 12.5 | 37.5
Impedance | (ohm) | 4 | 0.5 | 4 | 2 | 4 | 2
Size | (in) | 5.5×7.5 | 9 | 6×9 | 1 | 2 | 2 | 80 mm

  * :
Australian specs.