#
DISCHARGE HEADLIGHT CONTROL UNIT CONSTRUCTION/OPERATION

BHE091801052T05

  Warning

  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See Mazda RX-8 Workshop Manual (1796-1-*-03D).)

• Built into the headlight and installed on the headlight lower side.

1 | Discharge headlight control unit

• Switches the direct current from the battery to alternating current (25,000 V) and optimally controls the current supply output to the bulb.