#
OUTER MIRROR CONSTRUCTION

BHE091269100T04

• Built-in mirror glass adjusting motors have been adopted.

• A filament is attached to the rear side of the mirror glass.

• A built-in ground illumination light, which illuminates when the keyless entry system is activated or the doors are opened or closed, has been adopted. For details of the ground illumination system, refer to INTERIOR LIGHTING SYSTEM CONTROL SYSTEM OPERATION

1 | Left/right adjusting motor
2 | Up/down adjusting motor
3 | Ground illumination light bulb
4 | Filament