#
COMBINATION SWITCH DISASSEMBLY/ASSEMBLY

BHE091866120W02

  Caution

  • For vehicles with DSC: If the disc on the combination switch is deformed or has foreign material adhering to it, performance of the steering angle sensor may be reduced, causing abnormal operation. When handling the combination switch, be careful not to deform the disc and make sure there is no foreign material on it.

1. Disassemble in the order indicated in the table.

1 | Screw
2 | Wiper and washer switch (L.H.D.) /Light switch (R.H.D.)
3 | Light switch (L.H.D.) /Wiper and washer switch (R.H.D.)
4 | Body

2. Assemble in the reverse order of disassembly.