#
TRIPLE SYNCHRONIZER MECHANISM STRUCTURE [R15M-D]

BHE051101025T05

## Features

• A triple cone synchronizer mechanism is used for the 1st, 2nd and 3rd gears.

• The triple cone synchronizer mechanism is a compact device capable of heavy duty meshing.

• The synchro mechanism reduces meshing time and improves operation.

• The triple cone synchro mechanism includes a synchronizer ring, a double cone, and an inner cone.

## Structure

Structural view

1 | Double cone
2 | Inner cone
3 | 2nd gear
4 | Synchronizer ring
5 | Clutch hub
6 | Clutch hub sleeve