#
OIL SEAL (COMPANION FLANGE) REPLACEMENT

BHE031427141W02

1. Remove the rear differential. (See REAR DIFFERENTIAL REMOVAL/INSTALLATION.)

2. Replace the oil seal (companion flange) referring to the rear differential disassembly/assembly procedure. (See REAR DIFFERENTIAL DISASSEMBLY.) (See REAR DIFFERENTIAL ASSEMBLY.)

3. Install the rear differential. (See REAR DIFFERENTIAL REMOVAL/INSTALLATION.)