#
POWER SEAT CONSTRUCTION/OPERATION

BHE091357101T02

• The following motors are built into the seat:

  – Slide motor
  – Recliner motor
  – Front tilt motor
  – Rear tilt motor
  – Lumbar support motor

• The slide, front tilt and rear tilt switches are all operated by use of a single switch knob.

1 | Recliner operation
2 | Slide operation
3 | Front tilt operation
4 | Rear tilt operation
5 | Lumbar support operation
6 | Recliner motor
7 | Lumbar support motor
8 | Slide motor
9 | Front tilt motor
10 | Rear tilt motor
11 | Slide switch/Front tilt switch/Rear tilt switch
12 | Recliner switch
13 | Lumbar support switch