#
CONTROLLER AREA NETWORK (CAN) SYSTEM OUTLINE

BHE094055430T01

• Due to the simplification of the wiring harness, a CAN system for transmission of multiplex input/output signals among electrical modules has been adopted.

• Twisted-pair wiring is used for connections between the following modules. (Each electrical module hereafter referred to as a CAN system-related module):

  – PCM to TCM to DSC HU/CM to steering angle sensor to keyless unit to EPS control module to instrument cluster

• With an on-board diagnostic function included for each multiplex module, display of DTCs using the WDS or equivalent has improved serviceability.