#
AUTOMATIC TRANSMISSION SPECIFICATIONS

BHE050001030T07

Item | Specifications
--- | ---
Transmission type | RC4A-EL
Gear ratio | 1GR | 2.785
2GR | 1.545
3GR | 1.000
4GR | 0.694
Reverse | 2.272
ATF | Type | ATF M-III or equivalent (e.g. DexronII)
Capacity (Approx. quantity) (L {US qt, lmp qt}) | 8.7 {9.2, 7.7}
Torque converter stall torque ratio | 2.04: 1
Hydraulic system (Number of drive/driven plates) | Low clutch | 5/5
High clutch | 6/6
Reverse clutch | 2/2
2-4 brake | 4/8
Low and reverse brake | 4/5
Front planetary gear (Number of teeth) | Sun gear | 33
Pinion gear | 21
Internal gear | 75
Rear planetary gear (Number of teeth) | Sun gear | 42
Pinion gear | 17
Internal gear | 75