#
OIL PRESSURE SWITCH FUNCTION

BHE051319200T01

• The oil pressure switches detect pressure applied to the clutch and brakes, and sends control signals to the TCM.

• The TCM controls clutch engagement based on these signals.

• The oil pressure switches have the following functions:

Function chart

Oil pressure switch | Function
--- | ---
Oil pressure switch B | Detects pressure applied to 2-4 brake
Oil pressure switch C | Detects pressure applied to high clutch
Oil pressure switch F | Detects pressure applied to low and reverse brake

1 | Oil pressure switch C
2 | Oil pressure switch B
3 | Oil pressure switch F