#
CAR-NAVIGATION CONTROL SWITCH REMOVAL/INSTALLATION

BHE092066921W01

1. Disconnect the negative battery cable.

2. Remove the shift console. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Car-navigation control switch (See Car-Navigation Control Switch Removal Note.)
2 | Connector

4. Install in the reverse order of removal.

## Car-Navigation Control Switch Removal Note

1. Remove the car-navigation control switch while pressing tabs A as shown in the figure.