#
NO.27 ENGINE STALLS WHEN DRIVING AT SLOW SPEEDS OR STOPPING

BHE050301026W32

27 | Engine stalls when driving at slow speeds or stopping
DESCRIPTION | • Engine stalls when brake pedal is depressed while driving at low speed or stopping.
POSSIBLE CAUSE | • Malfunction in engine control system (e.g. fuel injection control, electronic throttle control system) Otherwise, the malfunction is in the control valve body, and/or TCC solenoid.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Go to symptom troubleshooting No.10 "LOW IDLE/STALLS DURING DECELERATION". (See NO.10 LOW IDLE/STALLS DURING DECELERATION.) Is the engine control system normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts according to inspection results.
2 | Go to symptom troubleshooting No.5 "ENGINE STALLS-AFTER START/AT IDLE". (See NO.5 ENGINE STALLS-AFTER START/AT IDLE.) Is the engine control system normal? | Yes | Repeat the basic inspection and repair or replace any malfunctioning parts according to the inspection result. (See BASIC INSPECTION.)
No | Repair or replace any malfunctioning parts according to the inspection results.
3 | Verify the test results. • If normal, return to the diagnostic index to service any additional symptoms. • If the malfunction remains, inspect the related Service Bulletins and/or On-line Repair Information and perform repair or diagnosis. – If the vehicle is repaired, troubleshooting completed. – If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM. (See TCM REMOVAL/INSTALLATION.)