#
BRAKE SPECIFICATIONS

BHE040001021T03

Item | Specification
--- | ---
Brake pedal | Type | Suspended design
Pedal lever ratio | 2.8
Max. stroke | (mm {in}) | 140 {5.51}
Master cylinder | Type | Tandem (plunger type)
Cylinder bore | (mm {in}) | 22.22 {0.875}
Front brake (disc) | Type | Ventilated disc
Cylinder bore | (mm {in}) | 54.0 {2.13}
Pad dimensions (area x thickness) | 4,840 x 11 {7.744 x 0.43}
(mm2 x mm {in2 x in})
Disc plate dimensions (outer diameter x thickness) | Standard suspension: 303 x 24 {11.9 x 0.94} Sport suspension: 323 x 24 {12.7 x 0.94}
(mm {in})
Rear brake (disc) | Type | Ventilated disc
Cylinder bore | (mm {in}) | 42.85 {1.687}
Pad dimensions (area x thickness) | 3,330 x 9 {5.328 x 0.4}
(mm2 x mm {in2 x in})
Disc plate dimensions (outer diameter x thickness) | 302 x 18 {11.9 x 0.71}
(mm {in})
Power brake unit | Type | Vacuum multiplier Single diaphragm
Outer diameter | (mm {in}) | 274 {10.8}
Rear wheel braking force control device | Type | EBD (Electronic brakeforce distribution)
Parking brake | Type | Mechanical two-rear-wheel control
Operation system | Center lever type
Brake fluid | Type | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT3 or DOT4 Australian specs.: SAE J1703, FMVSS 116 DOT3